


STEP1: 


STEP 2


S


STEP2 


STEP3


STEP4


STEP5


STEP6

STEP7

STEP8

STEP9

STEP10

STEP11

ADVANTAGES: ADD MORE SECURITY LAYER, COST FRIENDLY, CAN WORK ON ONE HARDWARE RATHER THAN MULTIPLE

DISADVANTAGES: COMPLEXITY, IT PUT CPU INTO MORE PRESSURE RESULT IN PROCESSOR HEATING, MAKE PC SLOW TO WORK AND REQUIRE MORE SPACE